# Configuration file for fw_(printenv/setenv) utility.
# Up to two entries are valid, in this case the redundant
# environment sector is assumed present.
# Notice, that the "Number of sectors" is not required on NOR and SPI-dataflash.
# Futhermore, if the Flash sector size is omitted, this value is assumed to
# be the same as the Environment size, which is valid for NOR and SPI-dataflash
# Device offset must be prefixed with 0x to be parsed as a hexadecimal value.

# UBI volume by name        Offset     Size     Erase-size
/dev/ubi0:uboot_config          0x0             0x20000         0x20000
/dev/ubi0:uboot_config_r        0x0             0x20000         0x20000
