
# Wi-Fi AP interface (NXP IW612)
#auto uap0
iface uap0 inet dhcp
       udhcpc_opts -S -b >/dev/null &
       pre-up [ -d /proc/device-tree/wireless ]
       post-up ##WLAN1_POST_UP_ACTION##
       pre-down ##WLAN1_PRE_DOWN_ACTION##
