From 69d18183a1df9e72371e33937c91af5b5b79a110 Mon Sep 17 00:00:00 2001
From: Chung-Hsien Hsu <chung-hsien.hsu@infineon.com>
Date: Mon, 2 Aug 2021 14:15:06 -0500
Subject: [PATCH 13/49] non-upstream: defconfig_base: Add Infineon default
 configuration

Add Infineon default configuration files (defconfig_base).

Signed-off-by: Kurt Lee <kurt.lee@infineon.com>
Signed-off-by: Chung-Hsien Hsu <chung-hsien.hsu@infineon.com>
---
 hostapd/defconfig_base        | 403 +++++++++++++++++++++
 wpa_supplicant/defconfig_base | 635 ++++++++++++++++++++++++++++++++++
 2 files changed, 1038 insertions(+)
 create mode 100644 hostapd/defconfig_base
 create mode 100644 wpa_supplicant/defconfig_base

diff --git a/hostapd/defconfig_base b/hostapd/defconfig_base
new file mode 100644
index 000000000..9dcf7848d
--- /dev/null
+++ b/hostapd/defconfig_base
@@ -0,0 +1,403 @@
+# Example hostapd build time configuration
+#
+# This file lists the configuration options that are used when building the
+# hostapd binary. All lines starting with # are ignored. Configuration option
+# lines must be commented out complete, if they are not to be included, i.e.,
+# just setting VARIABLE=n is not disabling that variable.
+#
+# This file is included in Makefile, so variables like CFLAGS and LIBS can also
+# be modified from here. In most cass, these lines should use += in order not
+# to override previous values of the variables.
+
+# Driver interface for Host AP driver
+CONFIG_DRIVER_HOSTAP=y
+
+# Driver interface for wired authenticator
+#CONFIG_DRIVER_WIRED=y
+
+# Driver interface for drivers using the nl80211 kernel interface
+CONFIG_DRIVER_NL80211=y
+
+# QCA vendor extensions to nl80211
+#CONFIG_DRIVER_NL80211_QCA=y
+
+# driver_nl80211.c requires libnl. If you are compiling it yourself
+# you may need to point hostapd to your version of libnl.
+#
+#CFLAGS += -I$<path to libnl include files>
+#LIBS += -L$<path to libnl library files>
+
+# Use libnl v2.0 (or 3.0) libraries.
+#CONFIG_LIBNL20=y
+
+# Use libnl 3.2 libraries (if this is selected, CONFIG_LIBNL20 is ignored)
+CONFIG_LIBNL32=y
+
+
+# Driver interface for FreeBSD net80211 layer (e.g., Atheros driver)
+#CONFIG_DRIVER_BSD=y
+#CFLAGS += -I/usr/local/include
+#LIBS += -L/usr/local/lib
+#LIBS_p += -L/usr/local/lib
+#LIBS_c += -L/usr/local/lib
+
+# Driver interface for no driver (e.g., RADIUS server only)
+#CONFIG_DRIVER_NONE=y
+
+# WPA2/IEEE 802.11i RSN pre-authentication
+CONFIG_RSN_PREAUTH=y
+
+# Support Operating Channel Validation
+#CONFIG_OCV=y
+
+# Integrated EAP server
+CONFIG_EAP=y
+
+# EAP Re-authentication Protocol (ERP) in integrated EAP server
+CONFIG_ERP=y
+
+# EAP-MD5 for the integrated EAP server
+CONFIG_EAP_MD5=y
+
+# EAP-TLS for the integrated EAP server
+CONFIG_EAP_TLS=y
+
+# EAP-MSCHAPv2 for the integrated EAP server
+CONFIG_EAP_MSCHAPV2=y
+
+# EAP-PEAP for the integrated EAP server
+CONFIG_EAP_PEAP=y
+
+# EAP-GTC for the integrated EAP server
+CONFIG_EAP_GTC=y
+
+# EAP-TTLS for the integrated EAP server
+CONFIG_EAP_TTLS=y
+
+# EAP-SIM for the integrated EAP server
+#CONFIG_EAP_SIM=y
+
+# EAP-AKA for the integrated EAP server
+#CONFIG_EAP_AKA=y
+
+# EAP-AKA' for the integrated EAP server
+# This requires CONFIG_EAP_AKA to be enabled, too.
+#CONFIG_EAP_AKA_PRIME=y
+
+# EAP-PAX for the integrated EAP server
+#CONFIG_EAP_PAX=y
+
+# EAP-PSK for the integrated EAP server (this is _not_ needed for WPA-PSK)
+#CONFIG_EAP_PSK=y
+
+# EAP-pwd for the integrated EAP server (secure authentication with a password)
+#CONFIG_EAP_PWD=y
+
+# EAP-SAKE for the integrated EAP server
+#CONFIG_EAP_SAKE=y
+
+# EAP-GPSK for the integrated EAP server
+#CONFIG_EAP_GPSK=y
+# Include support for optional SHA256 cipher suite in EAP-GPSK
+#CONFIG_EAP_GPSK_SHA256=y
+
+# EAP-FAST for the integrated EAP server
+#CONFIG_EAP_FAST=y
+
+# EAP-TEAP for the integrated EAP server
+# Note: The current EAP-TEAP implementation is experimental and should not be
+# enabled for production use. The IETF RFC 7170 that defines EAP-TEAP has number
+# of conflicting statements and missing details and the implementation has
+# vendor specific workarounds for those and as such, may not interoperate with
+# any other implementation. This should not be used for anything else than
+# experimentation and interoperability testing until those issues has been
+# resolved.
+#CONFIG_EAP_TEAP=y
+
+# Wi-Fi Protected Setup (WPS)
+CONFIG_WPS=y
+# Enable UPnP support for external WPS Registrars
+#CONFIG_WPS_UPNP=y
+# Enable WPS support with NFC config method
+#CONFIG_WPS_NFC=y
+
+# EAP-IKEv2
+#CONFIG_EAP_IKEV2=y
+
+# Trusted Network Connect (EAP-TNC)
+#CONFIG_EAP_TNC=y
+
+# EAP-EKE for the integrated EAP server
+#CONFIG_EAP_EKE=y
+
+# PKCS#12 (PFX) support (used to read private key and certificate file from
+# a file that usually has extension .p12 or .pfx)
+CONFIG_PKCS12=y
+
+# RADIUS authentication server. This provides access to the integrated EAP
+# server from external hosts using RADIUS.
+#CONFIG_RADIUS_SERVER=y
+
+# Build IPv6 support for RADIUS operations
+CONFIG_IPV6=y
+
+# IEEE Std 802.11r-2008 (Fast BSS Transition)
+CONFIG_IEEE80211R=y
+
+# Use the hostapd's IEEE 802.11 authentication (ACL), but without
+# the IEEE 802.11 Management capability (e.g., FreeBSD/net80211)
+#CONFIG_DRIVER_RADIUS_ACL=y
+
+# Wireless Network Management (IEEE Std 802.11v-2011)
+# Note: This is experimental and not complete implementation.
+#CONFIG_WNM=y
+
+# IEEE 802.11ac (Very High Throughput) support
+CONFIG_IEEE80211AC=y
+
+# IEEE 802.11ax HE support
+# Note: This is experimental and work in progress. The definitions are still
+# subject to change and this should not be expected to interoperate with the
+# final IEEE 802.11ax version.
+CONFIG_IEEE80211AX=y
+
+# Remove debugging code that is printing out debug messages to stdout.
+# This can be used to reduce the size of the hostapd considerably if debugging
+# code is not needed.
+#CONFIG_NO_STDOUT_DEBUG=y
+
+# Add support for writing debug log to a file: -f /tmp/hostapd.log
+# Disabled by default.
+CONFIG_DEBUG_FILE=y
+
+# Send debug messages to syslog instead of stdout
+#CONFIG_DEBUG_SYSLOG=y
+
+# Add support for sending all debug messages (regardless of debug verbosity)
+# to the Linux kernel tracing facility. This helps debug the entire stack by
+# making it easy to record everything happening from the driver up into the
+# same file, e.g., using trace-cmd.
+#CONFIG_DEBUG_LINUX_TRACING=y
+
+# Remove support for RADIUS accounting
+#CONFIG_NO_ACCOUNTING=y
+
+# Remove support for RADIUS
+#CONFIG_NO_RADIUS=y
+
+# Remove support for VLANs
+#CONFIG_NO_VLAN=y
+
+# Enable support for fully dynamic VLANs. This enables hostapd to
+# automatically create bridge and VLAN interfaces if necessary.
+#CONFIG_FULL_DYNAMIC_VLAN=y
+
+# Use netlink-based kernel API for VLAN operations instead of ioctl()
+# Note: This requires libnl 3.1 or newer.
+#CONFIG_VLAN_NETLINK=y
+
+# Remove support for dumping internal state through control interface commands
+# This can be used to reduce binary size at the cost of disabling a debugging
+# option.
+#CONFIG_NO_DUMP_STATE=y
+
+# Enable tracing code for developer debugging
+# This tracks use of memory allocations and other registrations and reports
+# incorrect use with a backtrace of call (or allocation) location.
+#CONFIG_WPA_TRACE=y
+# For BSD, comment out these.
+#LIBS += -lexecinfo
+#LIBS_p += -lexecinfo
+#LIBS_c += -lexecinfo
+
+# Use libbfd to get more details for developer debugging
+# This enables use of libbfd to get more detailed symbols for the backtraces
+# generated by CONFIG_WPA_TRACE=y.
+#CONFIG_WPA_TRACE_BFD=y
+# For BSD, comment out these.
+#LIBS += -lbfd -liberty -lz
+#LIBS_p += -lbfd -liberty -lz
+#LIBS_c += -lbfd -liberty -lz
+
+# hostapd depends on strong random number generation being available from the
+# operating system. os_get_random() function is used to fetch random data when
+# needed, e.g., for key generation. On Linux and BSD systems, this works by
+# reading /dev/urandom. It should be noted that the OS entropy pool needs to be
+# properly initialized before hostapd is started. This is important especially
+# on embedded devices that do not have a hardware random number generator and
+# may by default start up with minimal entropy available for random number
+# generation.
+#
+# As a safety net, hostapd is by default trying to internally collect
+# additional entropy for generating random data to mix in with the data
+# fetched from the OS. This by itself is not considered to be very strong, but
+# it may help in cases where the system pool is not initialized properly.
+# However, it is very strongly recommended that the system pool is initialized
+# with enough entropy either by using hardware assisted random number
+# generator or by storing state over device reboots.
+#
+# hostapd can be configured to maintain its own entropy store over restarts to
+# enhance random number generation. This is not perfect, but it is much more
+# secure than using the same sequence of random numbers after every reboot.
+# This can be enabled with -e<entropy file> command line option. The specified
+# file needs to be readable and writable by hostapd.
+#
+# If the os_get_random() is known to provide strong random data (e.g., on
+# Linux/BSD, the board in question is known to have reliable source of random
+# data from /dev/urandom), the internal hostapd random pool can be disabled.
+# This will save some in binary size and CPU use. However, this should only be
+# considered for builds that are known to be used on devices that meet the
+# requirements described above.
+#CONFIG_NO_RANDOM_POOL=y
+
+# Should we attempt to use the getrandom(2) call that provides more reliable
+# yet secure randomness source than /dev/random on Linux 3.17 and newer.
+# Requires glibc 2.25 to build, falls back to /dev/random if unavailable.
+#CONFIG_GETRANDOM=y
+
+# Should we use poll instead of select? Select is used by default.
+#CONFIG_ELOOP_POLL=y
+
+# Should we use epoll instead of select? Select is used by default.
+#CONFIG_ELOOP_EPOLL=y
+
+# Should we use kqueue instead of select? Select is used by default.
+#CONFIG_ELOOP_KQUEUE=y
+
+# Select TLS implementation
+# openssl = OpenSSL (default)
+# gnutls = GnuTLS
+# internal = Internal TLSv1 implementation (experimental)
+# linux = Linux kernel AF_ALG and internal TLSv1 implementation (experimental)
+# none = Empty template
+CONFIG_TLS=openssl
+CONFIG_TLS_ADD_DL=y
+
+# TLS-based EAP methods require at least TLS v1.0. Newer version of TLS (v1.1)
+# can be enabled to get a stronger construction of messages when block ciphers
+# are used.
+#CONFIG_TLSV11=y
+
+# TLS-based EAP methods require at least TLS v1.0. Newer version of TLS (v1.2)
+# can be enabled to enable use of stronger crypto algorithms.
+#CONFIG_TLSV12=y
+
+# Select which ciphers to use by default with OpenSSL if the user does not
+# specify them.
+#CONFIG_TLS_DEFAULT_CIPHERS="DEFAULT:!EXP:!LOW"
+
+# If CONFIG_TLS=internal is used, additional library and include paths are
+# needed for LibTomMath. Alternatively, an integrated, minimal version of
+# LibTomMath can be used. See beginning of libtommath.c for details on benefits
+# and drawbacks of this option.
+#CONFIG_INTERNAL_LIBTOMMATH=y
+#ifndef CONFIG_INTERNAL_LIBTOMMATH
+#LTM_PATH=/usr/src/libtommath-0.39
+#CFLAGS += -I$(LTM_PATH)
+#LIBS += -L$(LTM_PATH)
+#LIBS_p += -L$(LTM_PATH)
+#endif
+# At the cost of about 4 kB of additional binary size, the internal LibTomMath
+# can be configured to include faster routines for exptmod, sqr, and div to
+# speed up DH and RSA calculation considerably
+#CONFIG_INTERNAL_LIBTOMMATH_FAST=y
+
+# Interworking (IEEE 802.11u)
+# This can be used to enable functionality to improve interworking with
+# external networks.
+#CONFIG_INTERWORKING=y
+
+# Hotspot 2.0
+#CONFIG_HS20=y
+
+# Enable SQLite database support in hlr_auc_gw, EAP-SIM DB, and eap_user_file
+#CONFIG_SQLITE=y
+
+# Enable Fast Session Transfer (FST)
+#CONFIG_FST=y
+
+# Enable CLI commands for FST testing
+#CONFIG_FST_TEST=y
+
+# Testing options
+# This can be used to enable some testing options (see also the example
+# configuration file) that are really useful only for testing clients that
+# connect to this hostapd. These options allow, for example, to drop a
+# certain percentage of probe requests or auth/(re)assoc frames.
+CONFIG_TESTING_OPTIONS=y
+
+# Automatic Channel Selection
+# This will allow hostapd to pick the channel automatically when channel is set
+# to "acs_survey" or "0". Eventually, other ACS algorithms can be added in
+# similar way.
+#
+# Automatic selection is currently only done through initialization, later on
+# we hope to do background checks to keep us moving to more ideal channels as
+# time goes by. ACS is currently only supported through the nl80211 driver and
+# your driver must have survey dump capability that is filled by the driver
+# during scanning.
+#
+# You can customize the ACS survey algorithm with the hostapd.conf variable
+# acs_num_scans.
+#
+# Supported ACS drivers:
+# * ath9k
+# * ath5k
+# * ath10k
+#
+# For more details refer to:
+# http://wireless.kernel.org/en/users/Documentation/acs
+#
+#CONFIG_ACS=y
+
+# Multiband Operation support
+# These extensions facilitate efficient use of multiple frequency bands
+# available to the AP and the devices that may associate with it.
+#CONFIG_MBO=y
+
+# Client Taxonomy
+# Has the AP retain the Probe Request and (Re)Association Request frames from
+# a client, from which a signature can be produced which can identify the model
+# of client device like "Nexus 6P" or "iPhone 5s".
+#CONFIG_TAXONOMY=y
+
+# Fast Initial Link Setup (FILS) (IEEE 802.11ai)
+#CONFIG_FILS=y
+# FILS shared key authentication with PFS
+#CONFIG_FILS_SK_PFS=y
+
+# Include internal line edit mode in hostapd_cli. This can be used to provide
+# limited command line editing and history support.
+#CONFIG_WPA_CLI_EDIT=y
+
+# Opportunistic Wireless Encryption (OWE)
+# Experimental implementation of draft-harkins-owe-07.txt
+#CONFIG_OWE=y
+
+# Airtime policy support
+#CONFIG_AIRTIME_POLICY=y
+
+# Override default value for the wpa_disable_eapol_key_retries configuration
+# parameter. See that parameter in hostapd.conf for more details.
+#CFLAGS += -DDEFAULT_WPA_DISABLE_EAPOL_KEY_RETRIES=1
+
+# Wired equivalent privacy (WEP)
+# WEP is an obsolete cryptographic data confidentiality algorithm that is not
+# considered secure. It should not be used for anything anymore. The
+# functionality needed to use WEP is available in the current hostapd
+# release under this optional build parameter. This functionality is subject to
+# be completely removed in a future release.
+#CONFIG_WEP=y
+
+# Remove all TKIP functionality
+# TKIP is an old cryptographic data confidentiality algorithm that is not
+# considered secure. It should not be used anymore. For now, the default hostapd
+# build includes this to allow mixed mode WPA+WPA2 networks to be enabled, but
+# that functionality is subject to be removed in the future.
+#CONFIG_NO_TKIP=y
+
+# Simultaneous Authentication of Equals (SAE), WPA3-Personal
+CONFIG_SAE=y
+
+# Device Provisioning Protocol (DPP)
+CONFIG_DPP=y
diff --git a/wpa_supplicant/defconfig_base b/wpa_supplicant/defconfig_base
new file mode 100644
index 000000000..15daf0ad2
--- /dev/null
+++ b/wpa_supplicant/defconfig_base
@@ -0,0 +1,635 @@
+# Example wpa_supplicant build time configuration
+#
+# This file lists the configuration options that are used when building the
+# wpa_supplicant binary. All lines starting with # are ignored. Configuration
+# option lines must be commented out complete, if they are not to be included,
+# i.e., just setting VARIABLE=n is not disabling that variable.
+#
+# This file is included in Makefile, so variables like CFLAGS and LIBS can also
+# be modified from here. In most cases, these lines should use += in order not
+# to override previous values of the variables.
+
+
+# Uncomment following two lines and fix the paths if you have installed OpenSSL
+# or GnuTLS in non-default location
+#CFLAGS += -I/usr/local/openssl/include
+#LIBS += -L/usr/local/openssl/lib
+
+# Some Red Hat versions seem to include kerberos header files from OpenSSL, but
+# the kerberos files are not in the default include path. Following line can be
+# used to fix build issues on such systems (krb5.h not found).
+#CFLAGS += -I/usr/include/kerberos
+
+# Driver interface for generic Linux wireless extensions
+# Note: WEXT is deprecated in the current Linux kernel version and no new
+# functionality is added to it. nl80211-based interface is the new
+# replacement for WEXT and its use allows wpa_supplicant to properly control
+# the driver to improve existing functionality like roaming and to support new
+# functionality.
+CONFIG_DRIVER_WEXT=y
+
+# Driver interface for Linux drivers using the nl80211 kernel interface
+CONFIG_DRIVER_NL80211=y
+
+# QCA vendor extensions to nl80211
+#CONFIG_DRIVER_NL80211_QCA=y
+
+# driver_nl80211.c requires libnl. If you are compiling it yourself
+# you may need to point hostapd to your version of libnl.
+#
+#CFLAGS += -I$<path to libnl include files>
+#LIBS += -L$<path to libnl library files>
+
+# Use libnl v2.0 (or 3.0) libraries.
+#CONFIG_LIBNL20=y
+
+# Use libnl 3.2 libraries (if this is selected, CONFIG_LIBNL20 is ignored)
+CONFIG_LIBNL32=y
+
+
+# Driver interface for FreeBSD net80211 layer (e.g., Atheros driver)
+#CONFIG_DRIVER_BSD=y
+#CFLAGS += -I/usr/local/include
+#LIBS += -L/usr/local/lib
+#LIBS_p += -L/usr/local/lib
+#LIBS_c += -L/usr/local/lib
+
+# Driver interface for Windows NDIS
+#CONFIG_DRIVER_NDIS=y
+#CFLAGS += -I/usr/include/w32api/ddk
+#LIBS += -L/usr/local/lib
+# For native build using mingw
+#CONFIG_NATIVE_WINDOWS=y
+# Additional directories for cross-compilation on Linux host for mingw target
+#CFLAGS += -I/opt/mingw/mingw32/include/ddk
+#LIBS += -L/opt/mingw/mingw32/lib
+#CC=mingw32-gcc
+# By default, driver_ndis uses WinPcap for low-level operations. This can be
+# replaced with the following option which replaces WinPcap calls with NDISUIO.
+# However, this requires that WZC is disabled (net stop wzcsvc) before starting
+# wpa_supplicant.
+# CONFIG_USE_NDISUIO=y
+
+# Driver interface for wired Ethernet drivers
+CONFIG_DRIVER_WIRED=y
+
+# Driver interface for MACsec capable Qualcomm Atheros drivers
+#CONFIG_DRIVER_MACSEC_QCA=y
+
+# Driver interface for Linux MACsec drivers
+#CONFIG_DRIVER_MACSEC_LINUX=y
+
+# Driver interface for the Broadcom RoboSwitch family
+#CONFIG_DRIVER_ROBOSWITCH=y
+
+# Driver interface for no driver (e.g., WPS ER only)
+#CONFIG_DRIVER_NONE=y
+
+# Solaris libraries
+#LIBS += -lsocket -ldlpi -lnsl
+#LIBS_c += -lsocket
+
+# Enable IEEE 802.1X Supplicant (automatically included if any EAP method or
+# MACsec is included)
+CONFIG_IEEE8021X_EAPOL=y
+
+# EAP-MD5
+CONFIG_EAP_MD5=y
+
+# EAP-MSCHAPv2
+CONFIG_EAP_MSCHAPV2=y
+
+# EAP-TLS
+CONFIG_EAP_TLS=y
+
+# EAL-PEAP
+CONFIG_EAP_PEAP=y
+
+# EAP-TTLS
+CONFIG_EAP_TTLS=y
+
+# EAP-FAST
+#CONFIG_EAP_FAST=y
+
+# EAP-TEAP
+# Note: The current EAP-TEAP implementation is experimental and should not be
+# enabled for production use. The IETF RFC 7170 that defines EAP-TEAP has number
+# of conflicting statements and missing details and the implementation has
+# vendor specific workarounds for those and as such, may not interoperate with
+# any other implementation. This should not be used for anything else than
+# experimentation and interoperability testing until those issues has been
+# resolved.
+#CONFIG_EAP_TEAP=y
+
+# EAP-GTC
+CONFIG_EAP_GTC=y
+
+# EAP-OTP
+CONFIG_EAP_OTP=y
+
+# EAP-SIM (enable CONFIG_PCSC, if EAP-SIM is used)
+#CONFIG_EAP_SIM=y
+
+# Enable SIM simulator (Milenage) for EAP-SIM
+#CONFIG_SIM_SIMULATOR=y
+
+# EAP-PSK (experimental; this is _not_ needed for WPA-PSK)
+#CONFIG_EAP_PSK=y
+
+# EAP-pwd (secure authentication using only a password)
+#CONFIG_EAP_PWD=y
+
+# EAP-PAX
+#CONFIG_EAP_PAX=y
+
+# LEAP
+CONFIG_EAP_LEAP=y
+
+# EAP-AKA (enable CONFIG_PCSC, if EAP-AKA is used)
+#CONFIG_EAP_AKA=y
+
+# EAP-AKA' (enable CONFIG_PCSC, if EAP-AKA' is used).
+# This requires CONFIG_EAP_AKA to be enabled, too.
+#CONFIG_EAP_AKA_PRIME=y
+
+# Enable USIM simulator (Milenage) for EAP-AKA
+#CONFIG_USIM_SIMULATOR=y
+
+# EAP-SAKE
+#CONFIG_EAP_SAKE=y
+
+# EAP-GPSK
+#CONFIG_EAP_GPSK=y
+# Include support for optional SHA256 cipher suite in EAP-GPSK
+#CONFIG_EAP_GPSK_SHA256=y
+
+# EAP-TNC and related Trusted Network Connect support (experimental)
+#CONFIG_EAP_TNC=y
+
+# Wi-Fi Protected Setup (WPS)
+CONFIG_WPS=y
+# Enable WPS external registrar functionality
+#CONFIG_WPS_ER=y
+# Disable credentials for an open network by default when acting as a WPS
+# registrar.
+#CONFIG_WPS_REG_DISABLE_OPEN=y
+# Enable WPS support with NFC config method
+#CONFIG_WPS_NFC=y
+
+# EAP-IKEv2
+#CONFIG_EAP_IKEV2=y
+
+# EAP-EKE
+#CONFIG_EAP_EKE=y
+
+# MACsec
+#CONFIG_MACSEC=y
+
+# PKCS#12 (PFX) support (used to read private key and certificate file from
+# a file that usually has extension .p12 or .pfx)
+CONFIG_PKCS12=y
+
+# Smartcard support (i.e., private key on a smartcard), e.g., with openssl
+# engine.
+CONFIG_SMARTCARD=y
+
+# PC/SC interface for smartcards (USIM, GSM SIM)
+# Enable this if EAP-SIM or EAP-AKA is included
+#CONFIG_PCSC=y
+
+# Support HT overrides (disable HT/HT40, mask MCS rates, etc.)
+#CONFIG_HT_OVERRIDES=y
+
+# Support VHT overrides (disable VHT, mask MCS rates, etc.)
+#CONFIG_VHT_OVERRIDES=y
+
+# Development testing
+#CONFIG_EAPOL_TEST=y
+
+# Select control interface backend for external programs, e.g, wpa_cli:
+# unix = UNIX domain sockets (default for Linux/*BSD)
+# udp = UDP sockets using localhost (127.0.0.1)
+# udp6 = UDP IPv6 sockets using localhost (::1)
+# named_pipe = Windows Named Pipe (default for Windows)
+# udp-remote = UDP sockets with remote access (only for tests systems/purpose)
+# udp6-remote = UDP IPv6 sockets with remote access (only for tests purpose)
+# y = use default (backwards compatibility)
+# If this option is commented out, control interface is not included in the
+# build.
+CONFIG_CTRL_IFACE=y
+
+# Include support for GNU Readline and History Libraries in wpa_cli.
+# When building a wpa_cli binary for distribution, please note that these
+# libraries are licensed under GPL and as such, BSD license may not apply for
+# the resulting binary.
+#CONFIG_READLINE=y
+
+# Include internal line edit mode in wpa_cli. This can be used as a replacement
+# for GNU Readline to provide limited command line editing and history support.
+#CONFIG_WPA_CLI_EDIT=y
+
+# Remove debugging code that is printing out debug message to stdout.
+# This can be used to reduce the size of the wpa_supplicant considerably
+# if debugging code is not needed. The size reduction can be around 35%
+# (e.g., 90 kB).
+#CONFIG_NO_STDOUT_DEBUG=y
+
+# Remove WPA support, e.g., for wired-only IEEE 802.1X supplicant, to save
+# 35-50 kB in code size.
+#CONFIG_NO_WPA=y
+
+# Remove IEEE 802.11i/WPA-Personal ASCII passphrase support
+# This option can be used to reduce code size by removing support for
+# converting ASCII passphrases into PSK. If this functionality is removed, the
+# PSK can only be configured as the 64-octet hexstring (e.g., from
+# wpa_passphrase). This saves about 0.5 kB in code size.
+#CONFIG_NO_WPA_PASSPHRASE=y
+
+# Simultaneous Authentication of Equals (SAE), WPA3-Personal
+CONFIG_SAE=y
+
+# Disable scan result processing (ap_scan=1) to save code size by about 1 kB.
+# This can be used if ap_scan=1 mode is never enabled.
+#CONFIG_NO_SCAN_PROCESSING=y
+
+# Select configuration backend:
+# file = text file (e.g., wpa_supplicant.conf; note: the configuration file
+#	path is given on command line, not here; this option is just used to
+#	select the backend that allows configuration files to be used)
+# winreg = Windows registry (see win_example.reg for an example)
+CONFIG_BACKEND=file
+
+# Remove configuration write functionality (i.e., to allow the configuration
+# file to be updated based on runtime configuration changes). The runtime
+# configuration can still be changed, the changes are just not going to be
+# persistent over restarts. This option can be used to reduce code size by
+# about 3.5 kB.
+#CONFIG_NO_CONFIG_WRITE=y
+
+# Remove support for configuration blobs to reduce code size by about 1.5 kB.
+#CONFIG_NO_CONFIG_BLOBS=y
+
+# Select program entry point implementation:
+# main = UNIX/POSIX like main() function (default)
+# main_winsvc = Windows service (read parameters from registry)
+# main_none = Very basic example (development use only)
+#CONFIG_MAIN=main
+
+# Select wrapper for operating system and C library specific functions
+# unix = UNIX/POSIX like systems (default)
+# win32 = Windows systems
+# none = Empty template
+#CONFIG_OS=unix
+
+# Select event loop implementation
+# eloop = select() loop (default)
+# eloop_win = Windows events and WaitForMultipleObject() loop
+#CONFIG_ELOOP=eloop
+
+# Should we use poll instead of select? Select is used by default.
+#CONFIG_ELOOP_POLL=y
+
+# Should we use epoll instead of select? Select is used by default.
+#CONFIG_ELOOP_EPOLL=y
+
+# Should we use kqueue instead of select? Select is used by default.
+#CONFIG_ELOOP_KQUEUE=y
+
+# Select layer 2 packet implementation
+# linux = Linux packet socket (default)
+# pcap = libpcap/libdnet/WinPcap
+# freebsd = FreeBSD libpcap
+# winpcap = WinPcap with receive thread
+# ndis = Windows NDISUIO (note: requires CONFIG_USE_NDISUIO=y)
+# none = Empty template
+#CONFIG_L2_PACKET=linux
+
+# Disable Linux packet socket workaround applicable for station interface
+# in a bridge for EAPOL frames. This should be uncommented only if the kernel
+# is known to not have the regression issue in packet socket behavior with
+# bridge interfaces (commit 'bridge: respect RFC2863 operational state')').
+#CONFIG_NO_LINUX_PACKET_SOCKET_WAR=y
+
+# Support Operating Channel Validation
+#CONFIG_OCV=y
+
+# Select TLS implementation
+# openssl = OpenSSL (default)
+# gnutls = GnuTLS
+# internal = Internal TLSv1 implementation (experimental)
+# linux = Linux kernel AF_ALG and internal TLSv1 implementation (experimental)
+# none = Empty template
+#CONFIG_TLS=openssl
+
+# TLS-based EAP methods require at least TLS v1.0. Newer version of TLS (v1.1)
+# can be enabled to get a stronger construction of messages when block ciphers
+# are used. It should be noted that some existing TLS v1.0 -based
+# implementation may not be compatible with TLS v1.1 message (ClientHello is
+# sent prior to negotiating which version will be used)
+#CONFIG_TLSV11=y
+
+# TLS-based EAP methods require at least TLS v1.0. Newer version of TLS (v1.2)
+# can be enabled to enable use of stronger crypto algorithms. It should be
+# noted that some existing TLS v1.0 -based implementation may not be compatible
+# with TLS v1.2 message (ClientHello is sent prior to negotiating which version
+# will be used)
+#CONFIG_TLSV12=y
+
+# Select which ciphers to use by default with OpenSSL if the user does not
+# specify them.
+#CONFIG_TLS_DEFAULT_CIPHERS="DEFAULT:!EXP:!LOW"
+
+# If CONFIG_TLS=internal is used, additional library and include paths are
+# needed for LibTomMath. Alternatively, an integrated, minimal version of
+# LibTomMath can be used. See beginning of libtommath.c for details on benefits
+# and drawbacks of this option.
+#CONFIG_INTERNAL_LIBTOMMATH=y
+#ifndef CONFIG_INTERNAL_LIBTOMMATH
+#LTM_PATH=/usr/src/libtommath-0.39
+#CFLAGS += -I$(LTM_PATH)
+#LIBS += -L$(LTM_PATH)
+#LIBS_p += -L$(LTM_PATH)
+#endif
+# At the cost of about 4 kB of additional binary size, the internal LibTomMath
+# can be configured to include faster routines for exptmod, sqr, and div to
+# speed up DH and RSA calculation considerably
+#CONFIG_INTERNAL_LIBTOMMATH_FAST=y
+
+# Include NDIS event processing through WMI into wpa_supplicant/wpasvc.
+# This is only for Windows builds and requires WMI-related header files and
+# WbemUuid.Lib from Platform SDK even when building with MinGW.
+#CONFIG_NDIS_EVENTS_INTEGRATED=y
+#PLATFORMSDKLIB="/opt/Program Files/Microsoft Platform SDK/Lib"
+
+# Add support for new DBus control interface
+# (fi.w1.wpa_supplicant1)
+#CONFIG_CTRL_IFACE_DBUS_NEW=y
+
+# Add introspection support for new DBus control interface
+#CONFIG_CTRL_IFACE_DBUS_INTRO=y
+
+# Add support for loading EAP methods dynamically as shared libraries.
+# When this option is enabled, each EAP method can be either included
+# statically (CONFIG_EAP_<method>=y) or dynamically (CONFIG_EAP_<method>=dyn).
+# Dynamic EAP methods are build as shared objects (eap_*.so) and they need to
+# be loaded in the beginning of the wpa_supplicant configuration file
+# (see load_dynamic_eap parameter in the example file) before being used in
+# the network blocks.
+#
+# Note that some shared parts of EAP methods are included in the main program
+# and in order to be able to use dynamic EAP methods using these parts, the
+# main program must have been build with the EAP method enabled (=y or =dyn).
+# This means that EAP-TLS/PEAP/TTLS/FAST cannot be added as dynamic libraries
+# unless at least one of them was included in the main build to force inclusion
+# of the shared code. Similarly, at least one of EAP-SIM/AKA must be included
+# in the main build to be able to load these methods dynamically.
+#
+# Please also note that using dynamic libraries will increase the total binary
+# size. Thus, it may not be the best option for targets that have limited
+# amount of memory/flash.
+#CONFIG_DYNAMIC_EAP_METHODS=y
+
+# IEEE Std 802.11r-2008 (Fast BSS Transition) for station mode
+CONFIG_IEEE80211R=y
+
+# Add support for writing debug log to a file (/tmp/wpa_supplicant-log-#.txt)
+CONFIG_DEBUG_FILE=y
+
+# Send debug messages to syslog instead of stdout
+#CONFIG_DEBUG_SYSLOG=y
+# Set syslog facility for debug messages
+#CONFIG_DEBUG_SYSLOG_FACILITY=LOG_DAEMON
+
+# Add support for sending all debug messages (regardless of debug verbosity)
+# to the Linux kernel tracing facility. This helps debug the entire stack by
+# making it easy to record everything happening from the driver up into the
+# same file, e.g., using trace-cmd.
+#CONFIG_DEBUG_LINUX_TRACING=y
+
+# Add support for writing debug log to Android logcat instead of standard
+# output
+#CONFIG_ANDROID_LOG=y
+
+# Enable privilege separation (see README 'Privilege separation' for details)
+#CONFIG_PRIVSEP=y
+
+# Enable mitigation against certain attacks against TKIP by delaying Michael
+# MIC error reports by a random amount of time between 0 and 60 seconds
+#CONFIG_DELAYED_MIC_ERROR_REPORT=y
+
+# Enable tracing code for developer debugging
+# This tracks use of memory allocations and other registrations and reports
+# incorrect use with a backtrace of call (or allocation) location.
+#CONFIG_WPA_TRACE=y
+# For BSD, uncomment these.
+#LIBS += -lexecinfo
+#LIBS_p += -lexecinfo
+#LIBS_c += -lexecinfo
+
+# Use libbfd to get more details for developer debugging
+# This enables use of libbfd to get more detailed symbols for the backtraces
+# generated by CONFIG_WPA_TRACE=y.
+#CONFIG_WPA_TRACE_BFD=y
+# For BSD, uncomment these.
+#LIBS += -lbfd -liberty -lz
+#LIBS_p += -lbfd -liberty -lz
+#LIBS_c += -lbfd -liberty -lz
+
+# wpa_supplicant depends on strong random number generation being available
+# from the operating system. os_get_random() function is used to fetch random
+# data when needed, e.g., for key generation. On Linux and BSD systems, this
+# works by reading /dev/urandom. It should be noted that the OS entropy pool
+# needs to be properly initialized before wpa_supplicant is started. This is
+# important especially on embedded devices that do not have a hardware random
+# number generator and may by default start up with minimal entropy available
+# for random number generation.
+#
+# As a safety net, wpa_supplicant is by default trying to internally collect
+# additional entropy for generating random data to mix in with the data fetched
+# from the OS. This by itself is not considered to be very strong, but it may
+# help in cases where the system pool is not initialized properly. However, it
+# is very strongly recommended that the system pool is initialized with enough
+# entropy either by using hardware assisted random number generator or by
+# storing state over device reboots.
+#
+# wpa_supplicant can be configured to maintain its own entropy store over
+# restarts to enhance random number generation. This is not perfect, but it is
+# much more secure than using the same sequence of random numbers after every
+# reboot. This can be enabled with -e<entropy file> command line option. The
+# specified file needs to be readable and writable by wpa_supplicant.
+#
+# If the os_get_random() is known to provide strong random data (e.g., on
+# Linux/BSD, the board in question is known to have reliable source of random
+# data from /dev/urandom), the internal wpa_supplicant random pool can be
+# disabled. This will save some in binary size and CPU use. However, this
+# should only be considered for builds that are known to be used on devices
+# that meet the requirements described above.
+#CONFIG_NO_RANDOM_POOL=y
+
+# Should we attempt to use the getrandom(2) call that provides more reliable
+# yet secure randomness source than /dev/random on Linux 3.17 and newer.
+# Requires glibc 2.25 to build, falls back to /dev/random if unavailable.
+#CONFIG_GETRANDOM=y
+
+# IEEE 802.11ac (Very High Throughput) support (mainly for AP mode)
+CONFIG_IEEE80211AC=y
+
+# IEEE 802.11ax HE support (mainly for AP mode)
+# Note: This is experimental and work in progress. The definitions are still
+# subject to change and this should not be expected to interoperate with the
+# final IEEE 802.11ax version.
+CONFIG_IEEE80211AX=y
+
+# Wireless Network Management (IEEE Std 802.11v-2011)
+# Note: This is experimental and not complete implementation.
+#CONFIG_WNM=y
+
+# Interworking (IEEE 802.11u)
+# This can be used to enable functionality to improve interworking with
+# external networks (GAS/ANQP to learn more about the networks and network
+# selection based on available credentials).
+#CONFIG_INTERWORKING=y
+
+# Hotspot 2.0
+#CONFIG_HS20=y
+
+# Enable interface matching in wpa_supplicant
+#CONFIG_MATCH_IFACE=y
+
+# Disable roaming in wpa_supplicant
+#CONFIG_NO_ROAMING=y
+
+# AP mode operations with wpa_supplicant
+# This can be used for controlling AP mode operations with wpa_supplicant. It
+# should be noted that this is mainly aimed at simple cases like
+# WPA2-Personal while more complex configurations like WPA2-Enterprise with an
+# external RADIUS server can be supported with hostapd.
+#CONFIG_AP=y
+
+# P2P (Wi-Fi Direct)
+# This can be used to enable P2P support in wpa_supplicant. See README-P2P for
+# more information on P2P operations.
+CONFIG_P2P=y
+
+# Enable TDLS support
+#CONFIG_TDLS=y
+
+# Wi-Fi Display
+# This can be used to enable Wi-Fi Display extensions for P2P using an external
+# program to control the additional information exchanges in the messages.
+#CONFIG_WIFI_DISPLAY=y
+
+# Autoscan
+# This can be used to enable automatic scan support in wpa_supplicant.
+# See wpa_supplicant.conf for more information on autoscan usage.
+#
+# Enabling directly a module will enable autoscan support.
+# For exponential module:
+#CONFIG_AUTOSCAN_EXPONENTIAL=y
+# For periodic module:
+#CONFIG_AUTOSCAN_PERIODIC=y
+
+# Password (and passphrase, etc.) backend for external storage
+# These optional mechanisms can be used to add support for storing passwords
+# and other secrets in external (to wpa_supplicant) location. This allows, for
+# example, operating system specific key storage to be used
+#
+# External password backend for testing purposes (developer use)
+#CONFIG_EXT_PASSWORD_TEST=y
+
+# Enable Fast Session Transfer (FST)
+#CONFIG_FST=y
+
+# Enable CLI commands for FST testing
+#CONFIG_FST_TEST=y
+
+# OS X builds. This is only for building eapol_test.
+#CONFIG_OSX=y
+
+# Automatic Channel Selection
+# This will allow wpa_supplicant to pick the channel automatically when channel
+# is set to "0".
+#
+# TODO: Extend parser to be able to parse "channel=acs_survey" as an alternative
+# to "channel=0". This would enable us to eventually add other ACS algorithms in
+# similar way.
+#
+# Automatic selection is currently only done through initialization, later on
+# we hope to do background checks to keep us moving to more ideal channels as
+# time goes by. ACS is currently only supported through the nl80211 driver and
+# your driver must have survey dump capability that is filled by the driver
+# during scanning.
+#
+# TODO: In analogy to hostapd be able to customize the ACS survey algorithm with
+# a newly to create wpa_supplicant.conf variable acs_num_scans.
+#
+# Supported ACS drivers:
+# * ath9k
+# * ath5k
+# * ath10k
+#
+# For more details refer to:
+# http://wireless.kernel.org/en/users/Documentation/acs
+#CONFIG_ACS=y
+
+# Support Multi Band Operation
+#CONFIG_MBO=y
+
+# Fast Initial Link Setup (FILS) (IEEE 802.11ai)
+#CONFIG_FILS=y
+# FILS shared key authentication with PFS
+#CONFIG_FILS_SK_PFS=y
+
+# Support RSN on IBSS networks
+# This is needed to be able to use mode=1 network profile with proto=RSN and
+# key_mgmt=WPA-PSK (i.e., full key management instead of WPA-None).
+#CONFIG_IBSS_RSN=y
+
+# External PMKSA cache control
+# This can be used to enable control interface commands that allow the current
+# PMKSA cache entries to be fetched and new entries to be added.
+#CONFIG_PMKSA_CACHE_EXTERNAL=y
+
+# Mesh Networking (IEEE 802.11s)
+#CONFIG_MESH=y
+
+# Background scanning modules
+# These can be used to request wpa_supplicant to perform background scanning
+# operations for roaming within an ESS (same SSID). See the bgscan parameter in
+# the wpa_supplicant.conf file for more details.
+# Periodic background scans based on signal strength
+#CONFIG_BGSCAN_SIMPLE=y
+# Learn channels used by the network and try to avoid bgscans on other
+# channels (experimental)
+#CONFIG_BGSCAN_LEARN=y
+
+# Opportunistic Wireless Encryption (OWE)
+# Experimental implementation of draft-harkins-owe-07.txt
+#CONFIG_OWE=y
+
+# Device Provisioning Protocol (DPP)
+CONFIG_DPP=y
+
+# Wired equivalent privacy (WEP)
+# WEP is an obsolete cryptographic data confidentiality algorithm that is not
+# considered secure. It should not be used for anything anymore. The
+# functionality needed to use WEP is available in the current wpa_supplicant
+# release under this optional build parameter. This functionality is subject to
+# be completely removed in a future release.
+#CONFIG_WEP=y
+
+# Remove all TKIP functionality
+# TKIP is an old cryptographic data confidentiality algorithm that is not
+# considered secure. It should not be used anymore for anything else than a
+# backwards compatibility option as a group cipher when connecting to APs that
+# use WPA+WPA2 mixed mode. For now, the default wpa_supplicant build includes
+# support for this by default, but that functionality is subject to be removed
+# in the future.
+#CONFIG_NO_TKIP=y
+
+# Testing options
+# This can be used to enable some testing options (see also the example
+# configuration file) that are really useful only for testing clients that
+# connect to this hostapd. These options allow, for example, to drop a
+# certain percentage of probe requests or auth/(re)assoc frames.
+CONFIG_TESTING_OPTIONS=y
-- 
2.17.1

