#!/bin/sh
#===============================================================================
#
#  Copyright (C) 2023 by Digi International Inc.
#  All rights reserved.
#
#  This program is free software; you can redistribute it and/or modify it
#  under the terms of the GNU General Public License version 2 as published by
#  the Free Software Foundation.
#
#
#  !Description: Initialize bluetooth hardware
#
#===============================================================================

HCI_IFACE="hci0"
MODULE_NAME="btnxpuart"

log() {
	printf "<3>iw61x-bluetooth: %s\n" "${1}" >/dev/kmsg
}

# The power of the IW61x chip is managed by the WiFi DT entry.
#  If WiFi is disabled, is needed to manage the power manually.
is_not_wifi() {
	! [ -e "/proc/device-tree/wireless/mac-address" ]
}

power() {
	is_not_wifi && gpioset 1 7="${1}"
}

set_btaddr() {
	hciconfig ${HCI_IFACE} up
	sleep 0.2
	bt_addr=$(echo "$(fw_printenv -n btaddr)" | awk -F ":" '{ for(i=NF;i>=1;i--) printf "0x%s ", $i }')
	hcitool -i ${HCI_IFACE} cmd 0x3f 0x0022 0xfe 0x06 ${bt_addr}
	hciconfig ${HCI_IFACE} down
	sleep 0.2
	hciconfig ${HCI_IFACE} up
}

is_kernel_module_loaded() {
	lsmod | grep -qs -w "^${MODULE_NAME}"
}

bluetooth_start() {
	if ! [ -e "/proc/device-tree/bluetooth/mac-address" ]; then
		log "[ERROR] Bluetooth mac-address not found"
		return
	fi

	# If module is already loaded, skip
	is_kernel_module_loaded && log "[ERROR] kernel module already present, skipping" && return 1

	power 0 && sleep 0.2 && power 1
	# Load manually the kernel module
	modprobe "${MODULE_NAME}"
	# Reconfigure the HCI interface with the expected MAC address
	is_kernel_module_loaded && set_btaddr && log "Bluetooth activated" && return 0
	log "[ERROR] Cannot initialize Bluetooth correctly" && return 1
}

bluetooth_stop() {
	# Remove the kernel module
	rmmod "${MODULE_NAME}"
	power 0
}

case "$1" in
	start)
		bluetooth_start
		;;
	stop)
		bluetooth_stop
		;;
	restart)
		$0 stop
		$0 start
		;;
	*)
		echo "Usage: $0 {start|stop|restart}"
		exit 1
		;;
esac
