From: Javier Viguera <javier.viguera@digi.com>
Date: Thu, 20 Oct 2022 17:04:37 +0200
Subject: [PATCH] ccimx93: use UART6 for the default console

Signed-off-by: Javier Viguera <javier.viguera@digi.com>
---
 plat/imx/imx93/include/platform_def.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/plat/imx/imx93/include/platform_def.h b/plat/imx/imx93/include/platform_def.h
index 9bbee908fe80..8eba2f6d917a 100644
--- a/plat/imx/imx93/include/platform_def.h
+++ b/plat/imx/imx93/include/platform_def.h
@@ -61,7 +61,7 @@
 #define MAX_MMAP_REGIONS		17
 #endif
 
-#define IMX_LPUART_BASE			0x44380000
+#define IMX_LPUART_BASE			0x425a0000
 #define IMX_BOOT_UART_CLK_IN_HZ		24000000 /* Select 24MHz oscillator */
 #define IMX_CONSOLE_BAUDRATE		115200
 
