From: Arturo Buzarra <arturo.buzarra@digi.com>
Date: Tue, 16 Nov 2021 15:44:20 +0100
Subject: [PATCH] lib: set ATECC508A as default device type in default
 configuration

https://onedigi.atlassian.net/browse/DEL-7727

Signed-off-by: Arturo Buzarra <arturo.buzarra@digi.com>
---
 lib/atca_cfgs.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/lib/atca_cfgs.c b/lib/atca_cfgs.c
index 60727f71..1c875584 100644
--- a/lib/atca_cfgs.c
+++ b/lib/atca_cfgs.c
@@ -49,11 +49,11 @@
 #endif

 /** \brief default configuration for an ECCx08A device */
 ATCAIfaceCfg cfg_ateccx08a_i2c_default = {
     .iface_type             = ATCA_I2C_IFACE,
-    .devtype                = ATECC608A,
+    .devtype                = ATECC508A,
     .atcai2c.slave_address  = 0xC0,
     .atcai2c.bus            = ATCA_HAL_I2C_BUS,
     .atcai2c.baud           = ATCA_HAL_I2C_SPEED,
     //.atcai2c.baud = 100000,
     .wake_delay             = 1500,
