ACTION!="add|change|move", GOTO="mm_digi_xbee_cellular_modem_end"

# By default, ModemManager expects a default baudrate of 57600bps. Different
# baudrates may be used by setting the ID_MM_TTY_BAUDRATE udev tag.

# ModemManager documentation states that the best practice is to use the DEVPATH
# this way rather than other rules such as KERNEL, so be careful when modifying
DEVPATH=="/devices/soc0/soc.0/2100000.aips-bus/21f4000.serial/tty/ttymxc4", ENV{ID_MM_PLATFORM_DRIVER_PROBE}="1", ENV{ID_MM_PHYSDEV_UID}="Digi XBee Cellular"
DEVPATH=="/devices/soc0/soc/2100000.aips-bus/21f4000.serial/tty/ttymxc4", ENV{ID_MM_PLATFORM_DRIVER_PROBE}="1", ENV{ID_MM_PHYSDEV_UID}="Digi XBee Cellular"

LABEL="mm_digi_xbee_cellular_modem_end"
