ACTION!="add|change|move", GOTO="mm_digi_xbee_cellular_modem_end"

# By default, ModemManager expects a default baudrate of 57600bps. Different
# baudrates may be used by setting the ID_MM_TTY_BAUDRATE udev tag.

# ModemManager documentation states that the best practice is to use the DEVPATH
# this way rather than other rules such as KERNEL, so be careful when modifying
DEVPATH=="/devices/platform/5a800000.i2c/i2c-0/0-0063/mca-cc8x-uart/tty/ttyMCA0", ENV{ID_MM_PLATFORM_DRIVER_PROBE}="1", ENV{ID_MM_PHYSDEV_UID}="Digi XBee Cellular"

LABEL="mm_digi_xbee_cellular_modem_end"
