ctrl_interface=/var/run/wpa_supplicant
ctrl_interface_group=0
fast_reauth=1
update_config=1

## -- Example MANAGED network
ap_scan=1	# MANAGED mode
network={
	scan_ssid=1
	ssid=""
	key_mgmt=NONE
}

# -- SoftAP mode
# ap_scan=2
# network={
# 	ssid="ath6kl-ap"
# 	mode=2
# 	frequency=2412
# 	key_mgmt=WPA-PSK
# 	proto=RSN
# 	pairwise=CCMP
# 	psk="12345678"
# }
