
## Example bridge between eth0 and wlan0
#auto br0
#iface br0 inet static
#	bridge_ports eth0 wlan0
#	address 192.168.42.50
#	netmask 255.255.255.0
#	bridge_wpa_driver nl80211
#	bridge_wpa_conf /etc/wpa_supplicant.conf
