#
# U-Boot bootscript for NAND images created by Yocto.
#

#
# Set device tree filename depending on the board ID (if defined)
#
if test -n "${board_id}"; then
	setenv fdt_file zImage-imx6ul-ccimx6ulstarter-id${board_id}.dtb
else
	#
	# Set device tree filename depending on the hardware variant
	#
	if test "${module_variant}" = "0x02" || test "${module_variant}" = "0x04"; then
		setenv fdt_file zImage-imx6ul-ccimx6ulstarter-wb.dtb
	elif test "${module_variant}" = "0x03"; then
		setenv fdt_file zImage-imx6ul-ccimx6ulstarter.dtb
	else
		echo "------ Using default fdt_file: $fdt_file"
	fi
fi

if test "${mtdbootpart}" = "recovery"; then
	setenv boot_initrd true
	setenv initrd_file uramdisk-recovery.img
else
	true
fi
dboot linux nand ${mtdbootpart}
