From: Arturo Buzarra <arturo.buzarra@digi.com>
Date: Thu, 29 Apr 2021 15:02:19 +0200
Subject: [PATCH] imx8mm: Define UART1 as console for boot stage

UART1 is the default console for ConnectCore i.MX8M Mini

Signed-off-by: Arturo Buzarra <arturo.buzarra@digi.com>
Signed-off-by: Gabriel Valcazar <gabriel.valcazar@digi.com>
---
 plat/imx/imx8m/imx8mm/platform.mk | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/plat/imx/imx8m/imx8mm/platform.mk b/plat/imx/imx8m/imx8mm/platform.mk
index 83ebad65b..f47bdec22 100644
--- a/plat/imx/imx8m/imx8mm/platform.mk
+++ b/plat/imx/imx8m/imx8mm/platform.mk
@@ -62,7 +62,7 @@ $(eval $(call add_define,BL32_BASE))
 BL32_SIZE		?=	0x2000000
 $(eval $(call add_define,BL32_SIZE))
 
-IMX_BOOT_UART_BASE	?=	0x30890000
+IMX_BOOT_UART_BASE	?=	0x30860000
 $(eval $(call add_define,IMX_BOOT_UART_BASE))
 
 ifeq (${SPD},trusty)
