
## Example bridge between eth0 and wlan1 (Qualcomm QCA65x4)
#auto br0
#iface br0 inet static
#	bridge_ports eth0 wlan1
#	address 192.168.42.50
#	netmask 255.255.255.0
#	pre-up [ $(find /sys/devices -name modalias -print0 | xargs -0 sort -u -z | grep sdio:c00v0271d050A) ]
