From 7350cbc80f98eacb84a67049c2181f758ca3add6 Mon Sep 17 00:00:00 2001
From: Alex Gonzalez <alex.gonzalez@digi.com>
Date: Fri, 15 Jun 2018 09:18:15 +0200
Subject: [PATCH] imx6ul: Add MCA IOMUX support to the ConnectCore 6UL SOM

Synched with v4.14.78/master at.
3f8b03950b323db4ca89b1cdc1c2288f79facaa3

Signed-off-by: Alex Gonzalez <alex.gonzalez@digi.com>
---
 arch/arm/boot/dts/imx6ul-ccimx6ulsom.dtsi | 9 +++++++++
 1 file changed, 9 insertions(+)

diff --git a/arch/arm/boot/dts/imx6ul-ccimx6ulsom.dtsi b/arch/arm/boot/dts/imx6ul-ccimx6ulsom.dtsi
index 8d475051acf2..b96a0873cd88 100644
--- a/arch/arm/boot/dts/imx6ul-ccimx6ulsom.dtsi
+++ b/arch/arm/boot/dts/imx6ul-ccimx6ulsom.dtsi
@@ -286,6 +286,15 @@
 			MX6UL_PAD_SNVS_TAMPER9__GPIO5_IO09      0x3000
 		>;
 	};
+
+	pinctrl_mca_cc6ul: mcagrp {
+		fsl,pins = <
+			/* MCA_nINT */
+			MX6UL_PAD_SNVS_TAMPER4__GPIO5_IO04	0xb0b1
+			/* MCA_FW_UPDATE */
+			MX6UL_PAD_NAND_CE1_B__GPIO4_IO14	0x30
+		>;
+	};
 };
 
 &reg_arm {
