ACTION!="add|change|move|bind", GOTO="mm_net_device_blacklist_end"

# ModemManager documentation states that the best practice is to use the DEVPATH
# this way rather than other rules such as KERNEL, so be careful when modifying

# Remove CAN interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/platform/5a8e0000.can*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"
SUBSYSTEM=="net", DEVPATH=="/devices/platform/5a8f0000.can*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

# Remove Ethernet interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/platform/5b040000.ethernet*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"
SUBSYSTEM=="net", DEVPATH=="/devices/platform/5b050000.ethernet*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

# Remove PCIe interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/platform/5f010000.pcie*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

LABEL="mm_net_device_blacklist_end"
