From: Arturo Buzarra <arturo.buzarra@digi.com>
Date: Thu, 2 Apr 2020 16:26:48 +0200
Subject: [PATCH] wpa_supplicant: systemd: enable control socket interface for
 systemd service

Otherwise the command "wpa_cli" fails with:

Failed to connect to non-global ctrl_ifname

https://jira.digi.com/browse/DEL-6483

Signed-off-by: Arturo Buzarra <arturo.buzarra@digi.com>
---
 wpa_supplicant/systemd/wpa_supplicant.service.in | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/wpa_supplicant/systemd/wpa_supplicant.service.in b/wpa_supplicant/systemd/wpa_supplicant.service.in
index 58a622887cd9..cdc547f2ac5b 100644
--- a/wpa_supplicant/systemd/wpa_supplicant.service.in
+++ b/wpa_supplicant/systemd/wpa_supplicant.service.in
@@ -7,7 +7,7 @@ Wants=network.target
 [Service]
 Type=dbus
 BusName=fi.w1.wpa_supplicant1
-ExecStart=@BINDIR@/wpa_supplicant -u
+ExecStart=@BINDIR@/wpa_supplicant -u -O /var/run/wpa_supplicant
 
 [Install]
 WantedBy=multi-user.target
