ACTION!="add|change|move|bind", GOTO="mm_net_device_blacklist_end"

# ModemManager documentation states that the best practice is to use the DEVPATH
# this way rather than other rules such as KERNEL, so be careful when modifying

# Remove CAN interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/soc0/soc/2000000.aips-bus/2090000.flexcan*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"
SUBSYSTEM=="net", DEVPATH=="/devices/soc0/soc/2000000.aips-bus/2094000.flexcan*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

# Remove Ethernet interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/soc0/soc/2100000.aips-bus/2188000.ethernet*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

# Remove MMC interfaces from ModemManager probing
SUBSYSTEM=="net", DEVPATH=="/devices/soc0/soc/2100000.aips-bus/2190000.usdhc/mmc_host*", ENV{ID_MM_CANDIDATE}="0", ENV{ID_MM_DEVICE_IGNORE}="1"

LABEL="mm_net_device_blacklist_end"
